PERCEPTION-BASED SURVEY QUESTIONS 
FOR BICYCLE NETWORK AUDIT 2026

Surveyor Information
I. Survey Taken			: 
II. Surveyor Number		:
III. Block Number		:  
IV. How are you collecting the information? (Select only one)
a. Walking
b. Using a mobility aid 
c. Using a bicycle
d. Other

Survey Typology
V. What type of land uses are present in this block? (Select all that apply)
· UIUC campus institutional buildings
· Residential buildings
· Commercial or retail (shopping centers, restaurants, cafés)
· Industrial buildings (warehouses, factories)
· Parking lots or garages
· Designated green spaces/parks
· Underdeveloped land
· Vacant land
· Other

VI. What type of residential uses are present in this block? (Select all that apply)
· Single-family housing
· Multi-family housing 
· Apartments or condominiums 
· Apartments above street retail
· Retirement/senior living facility
· Dormitory
· Fraternity/sorority
· Other
· None

Safety
Bicycle Network 
1. Select all types of bicycle network infrastructure present in this block 
· Bicycle lane
· Off-street bicycle path
· Shared-use path with sidewalks more than 10 ft wide 
· Neighborhood greenway
· Sharrow or shared lanes
· Sidewalk 8-10 ft wide
· Sidewalk less than 8 ft wide
· Bicycle route with no 25 mph or lower marking 
· No bicycle facility
· Other 
	[image: Different Types Of Cycle Lane at Jo Perez blog]
Bicycle lane

	[image: All About the St. Paul Bicycle Plan - Streets.mn]
Off-street bicycle path
	[image: What can be done about overcrowded multi-use paths? - Canadian Cycling ...]
Shared-Use Path

	[image: Taking a ride on east Portland’s new neighborhood greenways – BikePortland]
Neighborhood greenway

	[image: River Street sharrows | Shared lane arrows or "sharrows" are… | Flickr]
Sharrow or shared lanes

	[image: Plans To Build 10-Foot-Wide Path Along Grand Boulevard Approved | New ...]
Sidewalk 8-10 ft wide

	[image: Rental Property Sidewalk Leveling - LevelUp Concrete Solutions]
Sidewalk less than 8 ft wide

	[image: 230+ British 20 Mph Speed Limit Traffic Sign Stock Photos, Pictures ...]
Bicycle route with no 25 mph or lower marking



2. How is the continuity of bicycle network from this block to the adjacent block(s)? 
· Transition is seamless because the bicycle network type remains the same in all directions
· Transition is mostly seamless because the bicycle network type remains the same in most direction, but changes in one or two blocks (E.g. transition from bike lane to shared-use path or vice versa)
· Transition is somewhat disrupted because bicyclists must change their direction or the bicycle network type in most adjacent blocks
· Transition is disrupted because bicyclists must change either their direction or the bicycle network type in all adjacent blocks
· Transition is highly disrupted because the bicycle network changes from a designated bicycle network to no bicycle facility (or vice versa) in most blocks
· No bicycle facility from all directions

3. If no bicycle lanes are present, is there any other place to bike that is safe from traffic?  (Select all that apply)
· No
· Yes – Bicycle lanes/path on the other side of the road
· Yes – Street Shoulder
· Yes – Buffer 
· Yes – Sidewalks
· Other 
· N/A – Bicycle lanes present on both sides of the street or off-street bike path continues in the zone
	[image: ODOT adds bike lanes to key section of N Lombard – BikePortland]
Bicycle lanes/path on the other side of the road
	[image: 8,400+ Road Shoulder Photos Stock Photos, Pictures & Royalty-Free ...]
Street shoulder


	[image: Council Demonstrated their Values in Emergency Road Funding - Raise the ...]
Buffer
	[image: Pedestrian Safety Is Behind McCormick’s Wider Walkways]
Sidewalks



Bicycle Markings 
4. Are bicycle markings present on the street? 
· Yes, markings are clearly visible 
· Yes, markings are somewhat visible 
· Yes, markings have faded
· No, markings are not present 

	[image: Premium Photo | White bike lane marking on an asphalt road road ...]
Visible markings
	[image: Bicycle Lane Marking Stock Photos, Images and Backgrounds for Free Download]
Fading markings



Bicycle Crosswalks
5. Are there bicycle crosswalks present on the street?
· Yes
· No
· Not applicable 

6. Are bicycle crosswalk markings present on the street? 
· Yes, markings are clearly visible 
· Yes, markings are somewhat visible 
· Yes, markings have faded
· No designated bicycle network 

	[image: crossbike and crosswalk childrens hospital protected bike … | Flickr]
Visible bicycle crosswalk
	[image: Salt causing crosswalks and traffic lines to fade | WWLP]
Fading bicycle crosswalk



Nighttime Safety Features
7. To what extent are the bicycle network lit in this block? 
· Well-lit with ample lighting (regularly spaced pedestrian lampposts)
· Somewhat lit with overhead streetlights on utility poles with wide spacing
· Not well lit 
· No lighting

Traffic Calming Measures 
8. What type of traffic calming measures are generally present in this block? (Select all that apply)
· Speed bumps 
· Curb extension
· Raised intersections and crosswalks
· Mid-block crosswalks without RRFB (rapid rectangular flashing beacons)
· Mid-block crosswalks with RRFB (rapid rectangular flashing beacons)
· Traffic diverters
· No traffic calming measures
· Other

	[image: Speed Bump In Spanish El Salvador at Nancy Guzman blog]
Speed bumps

	[image: 17th and 18th Avenues Bus Priority & Vision Zero Project - City and ...]
Curb extension

	[image: Types of Pedestrian Infrastructure]
Raised intersections and crosswalks

	[image: Rectangular Rapid-Flashing Beacon (RRFB) – TOMAR Traffic]
RRFB (Rapid Rectangular Flashing Beacons)
	[image: A diverter separates motor traffic from a bike lane ]
Traffic diverters

	



Bicycle Visibility 
9. Are bicyclists on bicycle networks easily visible and identifiable to pedestrians and/or other bicyclists?
· Yes, easily identifiable
· Low visibility
· Not visible

10. Are the bicyclists along the bike paths easily visible to vehicular traffic?  
· Yes, easily identifiable
· Low visibility
· Not visible

11. Are the bicyclists entering/exiting a crosswalk or intersection easily visible to vehicular traffic?  
· Yes, easily identifiable
· Low visibility
· Not visible

Bicycle Racks 
12. What is the general condition of bike racks in this block?	
· Very good 
· Good
· Need some improvement
· Need a lot of improvement
· No bike racks in this block

13. Are bicycle racks visible or noticeable while riding? 
· Always
· Most of the time 
· Sometimes
· Rarely
· None of the time 

14. How would you rate the level of bike racks usage? 
· 5 – Very high usage 
· 4 – High usage 
· 3 – Moderate usage
· 2 – Low usage 
· 1 – No usage

Path Quality
Path Size
15. Experts recommend that a one-way bike lane/path be at least 4 feet wide. Considering this recommendation, how would you rate the existing one-way bike path/lane width in this block, accounting for barriers that may reduce the width or make passing difficult? (Examples of barriers: Stationary -signal poles, fire hydrants, trees, utility poles; Moveable –planters, street signs, trees, furniture, mailboxes).
· Very adequate width 
· Adequate width
· Slightly narrow width
· Narrow width
· Very narrow width 
· No designated lane/path in this block 

Shared-use with Pedestrians
16. Traditional bicycles are allowed to operate on campus sidewalks. If a designated bicycle infrastructure is not present, could sidewalks accommodate occasional bicyclists during peak hour pedestrian traffic?
· Yes
· Needs to be wider
· Not observed during peak hour

17. In general, what is the overall condition of bicycle network infrastructure in this block?
· 5 – Excellent (Continuous bicycle network, well maintained and of sufficient width to accommodate bike traffic)
· 4 – Good (Bicycle network on both sides of the street)
· 3 – Need some improvements (Bicycle network on both sides of the street, minor discontinuities and maintenance problems but does not present major obstacles for bicycle)
· 2 – Need a lot of improvements (Bicycle network on one side of the road, several deficiencies)
· 1 – Poor (No permanent bicycle lane surfaces, discontinuous bicycle lane, or major maintenance problems)

Shades
18. To what extent are the bicycle lanes/paths shaded by trees in this block? 
· Well-shaded with regular intervals of trees
· Mostly shaded by trees 
· Somewhat shaded by trees
· No trees present 

Path Maintenance
19. Are there any obstructions in the bicycle network infrastructure in this block (Select all that apply)
· Drain gates 
· Utility covers 
· Metal plates 
· Rumble strips
· Temporary construction signage, equipment, or vehicles
· Vegetation growth obstructing the path 
· Other
· No dangerous obstructions
	[image: Types of Drain Grates - A Comprehensive Review | Paver shop]
Drain gates
	[image: WunderCovers - The Best Utility Access Covers]
Utility covers
	[image: Get to know more about Steel Road Plates - Sleepy Labeef]
Metal plates

	[image: 500MM YELLOW Plastic Rumble Strip - Speed Humps Australia]
Rumble strips


	[image: ]
Temporary construction signage, equipment, or vehicles
	[image: Grass growing in the cycle path © DS Pugh :: Geograph Britain and Ireland]
Vegetation growth obstructing the path




20. Are there any faults with the bicycle network infrastructure in this block? (Select all that apply)
· Potholes
· Uneven surfaces
· Too narrow 
· Major cracks
· Discontinuous path 
· Vegetation growth obstructing the path 
· No faults
· Other
	[image: 97,000+ Road Pothole Pictures]
Potholes
	[image: Uneven Surface Of Asphalt Road Stock Photo - Download Image Now ...]
Uneven surfaces
	[image: Narrow bike lanes at Collins and William Street | Cycling in… | Flickr]
Narrow lanes

	[image: L.A. City Repairing L.A. River Bike Path along Griffith Park ...]
Major cracks
	[image: STUPID IS AS STUPID DOES: Bike lane to nowhere in SD at the end of Governor  Drive at the I-805 on/off ramps. Runs into a fence and an area that is not]Discontinuous path
	[image: Grass growing in the cycle path © DS Pugh :: Geograph Britain and Ireland]
Vegetation growth obstructing the path



21. What do you think of the overall quality of the bicycle network maintenance? Consider things such as cracking, buckling, or standing water on or near bicycle lanes.
· 5 – Excellent (Bicycle networks are in excellent condition with no visible deficiencies)
· 4 – Very good (Bicycle networks are mostly in good condition with a few deficiencies)
· 3 – Good (Bicycle networks are mostly in good condition with several deficiencies)
· 2 – Bad (Bicycle networks are poorly maintained with many visible deficiencies but are generally bikeable)
· 1 – Very bad (Bicycle networks are poorly maintained with frequent or severe deficiencies, and are not bikeable)




Buffer
22. Please choose the average amount of space separating one-way bicycle lanes/paths from adjacent roadways. Choose the option that most closely matches your overall assessment of the buffers in this block.
· Excellent – Buffer is > 5 feet wide 
· Good – Buffer is 3-5 feet wide 
· Satisfactory – Buffer is < 3 feet wide
· Poor – No buffer from roadway
· Not applicable because the bicycle network type is sharrow

23. Please choose the average amount of space separating one-way bicycle lanes/paths from street parking. Choose the option that most closely matches your overall assessment of the buffers in this block
· Excellent – Buffer is > 5 feet from roadway 
· Good – Buffer is 3-5 feet wide 
· Satisfactory – Buffer is < 3 feet wide
· Poor – No buffer from street parking

Aesthetics
24. Which of the following amenities are available along the streets and bicycle network? Only select the ones easily identifiable by bicyclists
· Trees
· Green space
· Transit stops 
· Bicycle racks
· Bicycle repair station
· Air pump
· E-bike charging station
· Covered bike racks
· None of the above
· Other











	[image: Cycle Lanes Background Images, HD Pictures and Wallpaper For Free ...]
Trees
	[image: Bicycle Lane Along Side with Green Grass Meadow Field and Trees in ...]
Green space
	[image: First protected bike lane going up in 14th St. NW project - WTOP News]
Transit stops

	[image: Bike Transportation Engineers Paving the Way for Bicyclist-Safe Roads ...]
Bicycle racks
	[image: Bike repair stations help keep trail visitors rolling]
Bicycle repair station
	[image: Bicycle Repair Station And Air Pump at William Deas blog]
Air pump

	[image: World's First Network of Solar-Powered E-Bike Charging Stations | WE-cycle]
E-bike charging station
	[image: Your Expert UK Guide to Covered Bicycle Racks — Bison Products]
Covered bike racks
	



25. What do you think of the quality of aesthetics along this block? Consider things such as quality of landscaping, proximity to construction zones, fences, buildings, noise pollution, and bicycle-oriented features. Choose number that most closely matches your overall assessment of the aesthetics in this block.
· 5 – Very Pleasant (Visually inviting, quiet, landscaping, tree cover and architecture)
· 4 – Pleasant (Has minor deficiencies but a good block to bike)
· 3 – Average 
· 2 – Unpleasant (A good block to bike but has immense scope for improvement)
· 1 – Uninviting (I will not bike in this block again!)

Bicyclist Behavior
26. What kind of bicycles did you observe in this block? (Select all that apply) 
· Traditional bicycles
· E-bikes
· E-scooters/E-skateboards
· Veo Bikes
· Other micromobility devices 
· No bicycles are present 
	[image: ]
Traditional bicycles
	[image: Revv 1 Moped-Style Electric Bike | Ride1Up Ebikes]
E-bikes

	[image: 50 Miles Rang Adult Electric Scooter Dual SUSPENSION & BRAKES E Scooter ...]
E-scooter/E-skateboards
	[image: E-Scooter and E-Bike Sharing | Veo Micromobility]
Veo Bikes



27. Are bicyclists riding with helmets? 
· All bicyclists
· Most bicyclists
· Some bicyclists
· Few bicyclists
· No bicyclist
· I don’t know

28. Where are they mostly bicycling? 
· Riding on the sidewalk
· Riding on a bike lane or path 
· Riding on the shared use path
· Riding in the same direction as traffic
· Riding in the opposite direction as traffic 

29. How often do bicyclists: 
	
	5 - Always
	4 – Most of the time
	3 - Sometimes
	2 - Rarely
	1 – None of the time
	Not applicable

	Obeying stop lights
	
	
	
	
	
	

	Obeying stop signs
	
	
	
	
	
	

	Yielding to pedestrians on sidewalks and shared-use paths
	
	
	
	
	
	




Safety Perception
30. In general, how pleasant was your bike experience on this block? 
· 5 – Excellent
· 4 – Mostly satisfied
· 3 – Somewhat satisfied
· 2 – Needs considerable improvement
· 1 – I will not bike in this block again

31. How safe do you feel: 
	
	5 – Very safe
	4 – Safe
	3 – Somewhat safe
	2 – Unsafe
	1 - Stressed
	Not observed during this time

	When biking in this block during the day
	
	
	
	
	
	

	When biking in this block at night
	
	
	
	
	
	

	When biking in this block from crime, harassment, road rage, and other threats
	
	
	
	
	
	

	When crossing the road in this block with bicycle
	
	
	
	
	
	



32. Consider the speed, traffic volume, and visibility, how safe do you feel:
	
	5 – Very safe
	4 – Safe
	3 – Somewhat safe
	2 – Unsafe
	1 - Stressed

	When sharing the road with motorized vehicle
	
	
	
	
	

	When using the shared-use path with pedestrians
	
	
	
	
	

	When sharing the bicycle network with other bicyclist/E-scooter/other micromobility device users
	
	
	
	
	



Overall Quality 
33. What is your overall perception of the bicycle infrastructure on campus? 

34. What improvements would you like to see to enhance the campus bicycling experience? 
2
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